

* For this wall thickness parts, make sure that the cutter pushes the part into the vice. Benefits include:
	+ Better surface finish
	+ Less noise/chatter
	+ Tighter tolerance